**Technical Assistance Brief:**

**Assessing Lead-Based Paint Hazard Control Treatment Post-Remediation**

Attachment C.2: Dust Sample Collection

Date of Inspection: \_\_\_\_\_\_\_\_\_ (mm/dd/yy)

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Street No.** | **Street Name** | **Unit** | **City** | **State** | **ZIP Code** |
|  |  |  |  |  |  |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Room****Function** |  **Room** **Location** | **Sample**  **Type** |  **Sample Dimensions** |  **Sample**  **No.** | **Lead****(µg/sample)** | **Loading** **(µg/ft2)** |
|  **Length**  **(inches)** |  **Width** **(inches)** |
| Entry |  |  |  |  |  |  |  |
| Playroom |  |  |  |  |  |  |  |
| Playroom |  |  |  |  |  |  |  |
| Kitchen |  |  |  |  |  |  |  |
| Kitchen |  |  |  |  |  |  |  |
| Bedroom 1 |  |  |  |  |  |  |  |
| Bedroom 1 |  |  |  |  |  |  |  |
| Bedroom 2 |  |  |  |  |  |  |  |
| Bedroom 2 |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |

**Sample Type Code:** F = Floor, S = Windowsill, T = Window trough/well

Dust samples should be collected in accordance with the dust sampling protocols in the U.S. Department of Housing and Urban Development’s *Guidelines for the Evaluation and Control of Lead-Based Paint Hazards in Housing (2012 Edition)*. The dust sampling protocols can be found in Chapter 5, pages 5-35 through 5-49 at <http://portal.hud.gov/hudportal/documents/huddoc?id=ch05_12-13-12.pdf>.